Q1 driver package for Custom Engineering Spa Q1 dpi printer:

Windows 2000.
Windows XP.
Windows 2K3.

Installation procedure:

Serial, parallel and network interface
For (W2K, XP, W2K3) you must execute the standard printer installation procedure.

USB interface
Follow the automatic wizard procedure.

This driver support printer:
"Custom Q1"

The "Custom Q1" prints on a paper width size of 80mm but the printable
region width is 76mm.

This printer supports some page format:

"Q1 Roll"
"Q1 Roll Short"
"Q1 80mm"
"Q1 120mm"
"Q1 160mm"
"Q1 200mm"
"Q1 240mm"
"Q1 280mm"
"Q1 400mm"

If the system driver properties section shows these format pages and other not here
specified, you must select only the above mentioned pages format.

Note about BlackMark Feature:
 we suggest to use "Q1 Roll" page format when You are using Notch Alignmemnt.

